Zachary Harrington

This document explains the function of the Battery Charger, its schematic level design, and its board level design.

Battery Charger

Battery Charger Design

Revision: 1.0.0



Table of Contents

[1 Introduction 5](#_Toc132563178)

[1.1 Functions 5](#_Toc132563179)

[1.2 Requirements 5](#_Toc132563180)

[2 Detailed Description 6](#_Toc132563181)

[2.1 Functional Block Diagram 6](#_Toc132563182)

[2.1.1 Battery Charger 6](#_Toc132563183)

[2.1.2 Switching 6](#_Toc132563184)

[2.1.3 Batteries 6](#_Toc132563185)

[2.1.4 USB to UART 6](#_Toc132563186)

[2.1.5 PENIC 6](#_Toc132563187)

[2.1.6 Programmable LEDs 7](#_Toc132563188)

[2.1.7 External Control 7](#_Toc132563189)

[2.2 Schematic 7](#_Toc132563190)

[2.2.1 Battery Charger 7](#_Toc132563191)

[2.2.2 Charge Switching 9](#_Toc132563192)

[2.2.3 Protection Circuits 9](#_Toc132563193)

[2.2.4 USB to UART 9](#_Toc132563194)

[2.2.5 PENIC and 3.3V Voltage Regulation 10](#_Toc132563195)

[2.2.6 Programmable LEDs 11](#_Toc132563196)

[2.2.7 Isolated Grounds 11](#_Toc132563197)

[2.2.8 Connectors 11](#_Toc132563198)

[2.2.9 External Control 12](#_Toc132563199)

[2.3 Board 12](#_Toc132563200)

[2.3.1 Layout Constraints 12](#_Toc132563201)

[2.3.2 Battery Charger 13](#_Toc132563202)

[2.3.3 External Control 13](#_Toc132563203)

[2.3.4 DRC 13](#_Toc132563204)

[3 Testing 14](#_Toc132563205)

[3.1 Before First Power-On Check 14](#_Toc132563206)

[3.1.1 Test Instructions 14](#_Toc132563207)

[3.1.2 Test Data 14](#_Toc132563208)

[3.2 3.3V Regulator 14](#_Toc132563209)

[3.2.1 Test Instructions 15](#_Toc132563210)

[3.2.2 Test Data 15](#_Toc132563211)

[3.3 Charging Voltage 15](#_Toc132563212)

[3.3.1 Test Instructions 15](#_Toc132563213)

[3.3.2 Test Data 15](#_Toc132563214)

[3.4 Charging Current 15](#_Toc132563215)

[3.4.1 Test Instructions 15](#_Toc132563216)

[3.4.2 Test Data 15](#_Toc132563217)

[3.5 Battery Insertion 16](#_Toc132563218)

[3.5.1 Test Instructions 16](#_Toc132563219)

[3.5.2 Test Data 16](#_Toc132563220)

[3.6 Battery Charging 16](#_Toc132563221)

[3.6.1 Test Instructions 16](#_Toc132563222)

[3.6.2 Test Data 16](#_Toc132563223)

[3.7 External Control 16](#_Toc132563224)

[3.7.1 Test Instructions 17](#_Toc132563225)

[3.7.2 Test Data 17](#_Toc132563226)

[3.8 Charge Switching 17](#_Toc132563227)

[3.8.1 Test Instructions 17](#_Toc132563228)

[3.8.2 Test Data 17](#_Toc132563229)

[3.9 Battery Protection 18](#_Toc132563230)

[3.9.1 Overcharge 18](#_Toc132563231)

[3.9.2 Over-discharge 18](#_Toc132563232)

[3.9.3 Charge Overcurrent 19](#_Toc132563233)

[3.9.4 Discharge Overcurrent 19](#_Toc132563234)

[3.9.5 Load Short Circuit 20](#_Toc132563235)

[3.10 USB to UART Programming 21](#_Toc132563236)

[3.10.1 Test Instructions 21](#_Toc132563237)

[3.10.2 Test Data 21](#_Toc132563238)

[3.10.3 Test Notes 21](#_Toc132563239)

[3.11 Temperature Monitoring 21](#_Toc132563240)

[3.11.1 Test Instructions 21](#_Toc132563241)

[3.11.2 Test Data 21](#_Toc132563242)

[3.11.3 Test Notes 21](#_Toc132563243)

# Introduction

This document explains how the Battery Charger will fulfill the following Functions and conform to the following Requirements. This document refers to the Battery Charger version 1.0.

## Functions

The Battery Charger is responsible for the following:

* Charging up to three batteries on Earth
* Monitoring the charge status of each battery

## Requirements

1. Provide 4.2V 1.6A battery charging to up to three batteries in any order
2. Provide temperature and charge monitoring for each battery

# Detailed Description

This section refers to the Battery Charger schematic. Page numbers will be listed and may have coordinates listed (number and letter combination found around the frame).

## Functional Block Diagram

This section explains the high-level workings of the Battery Charger. The block diagram can be found on the first page of the schematic.

### Battery Charger

The charger IC regulates charging sourced from a 5V 3A wall adapter and charges lithium-ion batteries to 4.2V.

### Switching

Three ideal diodes control the flow of charge based on the charge status of each connected battery. The battery with the lowest voltage receives all the charging current until it is equal in voltage to another battery. Charging current is then split proportionally between all batteries of equal voltage, with higher charging currents being sent to batteries with higher capacities[[1]](#footnote-1).

### Batteries

Each battery is connected to a protection IC that protects against the following faults:

* Overcharge
* Over-discharge
* Charge overcurrent
* Discharge overcurrent
* Load short-circuit

The PENIC also monitors temperature through a thermistor next to each battery.

### USB to UART

The USB to UART IC is powered externally by the connected USB device. It provides USB to serial UART conversion to program and communicate with the PENIC.

### PENIC

The Performance and Error Notification IC (PENIC) is the microprocessor monitoring the status of the Battery Charger. The PENIC controls three programmable LEDs for visual feedback on the current charge status of each battery. Individual I/O pins read the status of the charger IC, each ideal diode, and each thermistor. Charge is cancelled for temperature faults through a direct connection to the charger IC.

A 3.3V 1A linear regulator steps down the 5V input to power the PENIC and all 3.3V references. All unused I/Os on the PENIC also connect to pins headers allowing for additional external sensors and components be monitored or ran by the PENIC. Four pin headers also connect to ground, 3.3V, and 5V to power external components. Each voltage rail supports a combined maximum of 0.5A. This maximum is not regulated and only defined by the available current not in use.

### Programmable LEDs

Three programmable LEDs display the current charge status of each battery. The color of each LED is defined by the PENIC and reflects the status of the respective battery[[2]](#footnote-2).

### External Control

Five physical switches serve as charge toggles. Three correspond to the three batteries, and two operate in unison to activate the charger itself. The PENIC is always active when connected to power and cannot be physically switched off.

## Schematic

This section explains the chosen circuit implementations and notable changes. The schematic drawings are found on pages two through five of the schematic.

### Battery Charger

The battery charger is implemented using the BQ24650[[3]](#footnote-3) battery charger IC (page 2, C2). This IC is designed with Maximum Power Point Tracking (MPPT), for use in variable voltage systems such as solar powered charging situations. It is implemented in this constant voltage system to gain experience designing with it and because the chips are already on-hand.

The battery charger sources power from the 5V 3A connector. At this input voltage the charger has an efficiency of between 80 and 90%.

Unless otherwise stated, the typical application layout from the BQ24650 IC documentation is used in this design. Notable changes are detailed below.

No single thermistor is used in this design because of the presence of three batteries. Rather, three thermistors are independently monitored by the PENIC, which is directly connected to the TS pin. During charging the TS pin voltage is kept between 2.43V and 1.485V, the high and low thresholds. In the event of a temperature fault, the TS pin is set to ground, 0V, and charge is cancelled until the TS pin is released or set to a voltage between 2.43V and 1.57V. Even with this protection, it is still recommended to not leave the batteries charging for long periods of time.

The output capacitance is the same, but on the schematic one of the capacitors can be seen moved slightly (page 2, C6) from the spot on the typical application (page 2, C5). Because it is connected to the same node, this has no net effect on the circuit and simply fits better on the schematic.

The inductor value is chosen to be 10µH to keep the LC resonant frequency between the recommended 12kHz to 17kHz, where the best stability occurs, as seen below:

The sense resistor is chosen to be 25mΩ to facilitate a charge current of 1.6A as seen below:

This current satisfies the maximum charge current of 1.625A required by the NCR168650B[[4]](#footnote-4) lithium-ion batteries that this charger is designed for. When more than one battery is being charged, a current less than this per battery is still acceptable.

The voltage divider between the output and VFB pin sets the max output voltage to 4.2V using 10kΩ resistors as seen below:

0Ω resistors are added to this voltage divider in the event extra precision or different values is needed.

One of the external control switches replaces the Charge Enable (CE) MOSFET from MPPSET to ground. When not actively switched to ground, MPPSET is held near 1.5V by the voltage divider, allowing the power to be unlimited. Any voltage over 1.2V effectively turns off MPPT, which is not needed in this constant voltage system.

D1 is implemented with a LTC4411[[5]](#footnote-5) ideal diode and serves as a redundancy to protect against reverse current from the batteries. It also is used for its control and status pins allowing the charge status to be monitored and controlled. In this case the control pin is connected to another external control switch and serves as an ON/OFF switch for the charger.

### Charge Switching

Switching is implemented using three LTC4411 ideal diodes (page 3, col 2). These diodes are connected in a parallel type of connection where any ratio of charge current can be passed to the three batteries. When any one battery has less voltage, and thus less charge than the rest, only that diode is biased and all the charging current flows to that battery. When instead multiple batteries have similar voltages, the corresponding diodes are all biased and the total charge current is split.

Input and output capacitors are added to each diode to reduce noise. While the input capacitors could be substituted with just one, given the nature of the high frequency switching in the charger IC and the possibility of the diodes not being in a central place on the board, one per diode is used.

A 475kΩ equivalent resistance is connected from each status pin to 3.3V so that the PENIC pin reads high when the diode is conducting, and thus the corresponding battery is charging. This resistance is considered to be an acceptable equivalent to the 470kΩ resistance recommended by the diode datasheet. It is also created from components already on-hand.

### Protection Circuits

Individual protection circuits for each battery are implemented using the BQ27900[[6]](#footnote-6) protection IC (page 4, A5, B5, & D3). While the charger IC contains protection circuits, the nature of switching between multiple batteries creates a need for individual protection ICs.

Unless otherwise stated, the typical application layout from the BQ29700 IC documentation is used in this design. Notable changes are detailed below.

The recommended 5MΩ resistors from COUT to ground and DOUT to VSS are implemented with 4.75MΩ resistors. This is considered to be an acceptable resistance and the resistors are already on-hand.

### USB to UART

A USB to UART serial data converter is implemented using the CP2102N[[7]](#footnote-7) IC (page 4, B3). This eliminates the need for an external converter to program the PENIC and creates a more user-friendly experience.

The IC sources power and programming data through the micro-USB cable connecter. This ensures the IC is powered only while data transfer is in progress. The use of a micro-USB connector helps differentiate between power and programming connections and matches with the current standard.

The CP2102N is capable of more than just USB to UART data conversion and thus no typical application was followed. Instead, unless otherwise stated, the diagram from PCB ARTISTS[[8]](#footnote-8) was used in this design. Notable changes are detailed below.

The 28-pin variant of the CP2102N is used for the TXT and RXT pins, which allow LEDs to be connected to visually display the TXD and RXD serial data transmission. 10kΩ resistors connect to each LED for similar brightness levels throughout the circuit.

An additional 4.7µF capacitor is added to the VDD pin as recommended by the datasheet.

As recommended, a 1ms RC time constant is added to the EN, and thus reset, pin. This is achieved using a 10kΩ resistor and 100nF capacitor (page 5, B2). The time constant ensures the IO0 pin has time to register LOW before the PENIC is toggled back on, telling it to boot in programming mode.

### PENIC and 3.3V Voltage Regulation

The Performance and Error Notification IC (PENIC) is an ESP32-S2-MINI-1[[9]](#footnote-9) microprocessor (page 5, C4). It was chosen for its low cost, integrated WI-FI antenna, and club members familiarity with programming it.

The IC sources power through the LD1117A[[10]](#footnote-10) (page 5, A1), a 3.3V 1A linear regulator which itself sources power through the 5V 3A connector. All I/O pins thus have a voltage level of 3.3V and any inputs must be stepped down to this.

The schematic application layout from the LD1117A datasheet is used in this design for 3.3V voltage regulation.

The peripheral schematics layout from the ESP32 documentation is used in this design for the RESET button, input voltage capacitors, and RC time constant discussed in the USB to UART section. Otherwise, all I/O pins are directly connected to their respective components, and a 10kΩ volage divider (page 5, C2) is used to read the thermistor data.

The NTCS0603E3T[[11]](#footnote-11) thermistor used has a room temperature resistance of 10kΩ, and a B25/85 value of 3960K. When the thermistor equation (4) is rearranged (5) the resistance at 85°C is found to be 1.08kΩ.

Temperatures in this equation are in Kelvin, though the B value may be denoted by the Celsius values. From these two values, an equation for the resistance of the thermistor vs. temperature can be obtained.

The batteries are rated between 10°C and 45°C during charging, making the acceptable voltage divider voltage range between 1.36V and 1.81V.

### Programmable LEDs

Three programmable LEDs are implemented using SK6812[[12]](#footnote-12) LEDs (page 5, A6 & B6). These LEDs require a 5V voltage level, and thus a bi-directional MOSFET level shifter[[13]](#footnote-13) (page5, A5) is implemented to step up the signal from the 3.3V ESP32 pin.

Without getting to detailed, see Electronics Hub[[14]](#footnote-14) for a full explanation, this level shifter circuit is implemented with a n-channel MOSFET containing a drain-substrate diode to ensure proper operation. Although this is not strictly necessary for this application of shifting to a higher voltage, it is still good practice and the NMOS is on-hand.

The typical application layout from the SK6812 datasheet is used in this design. Programming specifications are also located in the datasheet.

### Isolated Grounds

Three isolated grounds are used on this schematic. Power ground (PGND) is directly connected to the 5V 3A USB-C power connector ground. The other grounds are shorted to PGNDthrough 0Ω resistors rated up to 2A. Digital ground (DGND)connects to the CP2102N circuitry and the micro-USB connector. Chassis ground (CHASSIS) is connected to the mechanical features including the shields of the connectors.

### Connectors

There are three connectors, ways to add electrical input, on this device. Two are the 5V 3A USB-C power connector, and micro-USB programming connector. The other is the breakout pin headers for the PENIC (page 5, C2 & C5). All unused I/O pins are connected to a respective pin header in the event further monitoring or devices are added. Additionally, two PGND headers, a 3.3V 0.5A header, and a 5V 0.5A header are implemented to power these devices.

### External Control

The five control switches were implemented with large DPDT switches. This choice is simply for aesthetic and ergonomic reasons.

## Board

This section explains the chosen board layout and notable changes. The board layout is found in the Eagle board file. The board shall be double layered with 1 𝑜𝑧 copper and ENIG finish. The board has no dimension constraints and is 165mm x 75mm.

### Layout Constraints

Unless specified in the following subsections, all signals shall use the default parameters below. Signals in the following subsections do not include their sense signals unless otherwise specified. Trace width can be broken if a trace needs to bottleneck down to a pin, the bottleneck shall be minimized.

Trace width: 0.17𝑚𝑚

Vias: ∅0.35𝑚𝑚, unlimited count

Separation: 0.17𝑚𝑚

Length: unlimited

Devices with specific placement and routing considerations are called out on the schematic, see “CAD Note:”

#### Charger Power Traces – 5.0V, D1\_OUT, BQ24650\_[PH, SR\_P], CHARGER, D[3:5]\_OUT, BQ29700[1:3]\_VSS, PGND

5.0V applies to between the input connector and input diode. BQ24650\_PH applies to between the switching MOSFETs and inductor. BQ24650\_SR\_P applies to between the inductor and sense resistors. CHARGER applies to between the sense resistors and switching diodes. PGND applies to between the input diode and the three protection circuit MOSFETs.

Trace Width: 0.78mm

#### Pin Header Power Traces – 5.0V, PGND

5.0V applies to between the input diode, 3.3V regulator, and pin header. PGND applies to between the input connector and pin headers.

Trace width: 0.621mm

#### USB Differential Pair – D+, D-

Length: Length match ±1.0mm

Gap width: 0.375mm

#### 3.3V Regulator – 3.3V, PGND

3.3V applies to between the 3.3V regulator, pin header, and ESP32. PGND applies to between the 3.3V regulator and ESP32.

Trace width: 0.391mm

### Battery Charger

The layout guidelines from the BQ24650 charger IC datasheet are followed in this design.

### External Control

The external control switches are all placed next to each other for aesthetic and ease of use purposes. Although they are far from what they are controlling, since they are simply DC components, any noise or interference picked up on the traces isn’t an issue.

### DRC

Unless otherwise specified, all design rules checked by the DRC command were followed. Four clearance errors were approved for overlapping pads on the inductor footprint. Ten dimension errors were approved for the connectors needing to be in close proximity to the board edge. Four width errors were approved for the signature footprint.

# Testing

All tests shall be performed at room temperature and will not be performed under vacuum since the battery charger PCB will not be included on the actual satellite. If any modifications are performed, take note. Include enough information to understand circuit behavior and for others to replicate the results. Include any software written to execute the test and link it to the test notes section. Save all software, waveforms, etc. in a subfolder of the board’s test folder for each test. When testing, keep the following guidelines in mind:

* Waveforms shall be captured whenever appropriate
* Have the event take fill the screen (for fast events, zoom in, for slow events, zoom out)
* Label each channel accurately
* Only have bandwidth limiting if necessary for the test (this applies to the oscilloscope and probe settings)
* If ringing or overshoot occurs, use a ground spring or differential probe

Common test instructions can be found on the [wiki](https://cougs.space/wiki).

## Before First Power-On Check

**Configuration: Battery Charger V1.0.0**

This test is required to be executed before batteries are attached and before any external power is applied to the Battery Charger.

### Test Instructions

Measure the resistance of various points in reference to PGND located at test point 13 (TP13).

### Test Data

The data for this test will be recorded into the table below.

| Node | Resistance |  | Node | Resistance |
| --- | --- | --- | --- | --- |
| 5.0V (TP1) |  |  | TEMP\_B (TP8) |  |
| CHARGER (TP2) |  |  | TEMP\_C (TP9) |  |
| TS-ESP (TP3) |  |  | USB\_VDD (TP10) |  |
| D3\_OUT (TP4) |  |  | CP2102N\_VDD (TP11) |  |
| D4\_OUT (TP5) |  |  | 3.3V (TP12) |  |
| D5\_OUT (TP6) |  |  | PGND (TP13) | N/A |
| TEMP\_A (TP7) |  |  | D1\_OUT (TP14) |  |

## 3.3V Regulator

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in PENIC and 3.3V Voltage Regulation.

### Test Instructions

Connect a 5V 3A USB-C wall adapter to the board with all switches off.

### Test Data

| Measure the voltage at the 3.3V test point (TP12) | | |
| --- | --- | --- |
| Voltage | Passing Criteria | Pass / Fail |
|  |  |  |

## Charging Voltage

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in Battery Charger.

### Test Instructions

Connect a 5V 3A USB-C wall adapter to the board with all switches on. Apply various loads to the output and then measure the output voltage at the output connector.

### Test Data

| Voltage should be measured at the charger test point (TP2) | | | |
| --- | --- | --- | --- |
| Load | Voltage | Passing Criteria | Pass / Fail |
| No load |  |  |  |
| 500mA |  |  |  |

## Charging Current

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in Battery Charger.

### Test Instructions

Apply an increasing load to the output until the current no longer increases.

### Test Data

| Measure the current at one of the battery connectors | | |
| --- | --- | --- |
| Max current | Passing Criteria | Pass / Fail |
|  |  |  |

## Battery Insertion

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in Charge Switching.

### Test Instructions

Charge or discharge a battery to 3.7V before this test. Turn off all switches so no charge is flowing. Insert the battery into each connector and measure the voltage at the charger test point (TP2).

### Test Data

| Voltage should be measured at the charger test point (TP2) | | | |
| --- | --- | --- | --- |
| Battery | Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  |
| B |  |  |  |
| C |  |  |  |

## Battery Charging

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in Battery Charger.

### Test Instructions

Charge or discharge the batteries to 3.7V before this test. Connect a 5V 3A USB-C wall adapter to the board with all switches on. Insert all batteries and measure the change in voltage after 30 minutes to validate all batteries are charging.

### Test Data

| Measure the change in voltage after | | | | | |
| --- | --- | --- | --- | --- | --- |
| Battery | Initial Voltage | Final Voltage |  | Passing Criteria | Pass / Fail |
| A |  |  |  |  |  |
| B |  |  |  |  |  |
| C |  |  |  |  |  |

## External Control

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in External Control.

### Test Instructions

Charge or discharge the batteries to 3.7V before this test. Connect a 5V 3A USB-C wall adapter to the board with all switches on. Insert all batteries and measure the change in voltage in 30-minute intervals. For each interval only use one of the following configurations.

* Only Batt A On
* Only Batt B On
* Only Batt C On
* Batt A and B On
* Batt B and C On
* Batt C and A On

### Test Data

| Measure the change in voltage every | | | | | |
| --- | --- | --- | --- | --- | --- |
| Battery Configuration | Initial Voltage | Final Voltage |  | Passing Criteria | Pass / Fail |
| A |  |  |  |  |  |
| B |  |  |  |  |  |
| C |  |  |  |  |  |
| A, B |  |  |  |  |  |
| B, C |  |  |  |  |  |
| C, A |  |  |  |  |  |

## Charge Switching

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in Charge Switching.

### Test Instructions

Charge or discharge the batteries to 3.7V, 3.6V, and 3.5V respectively before this test. Connect a 5V 3A USB-C wall adapter to the board with all switches on. Insert all batteries and measure the change in voltage in 30-minute intervals. Validate only the batteries at the lowest voltage are charging at any given point.

### Test Data

| Measure the voltages every | | | | | |
| --- | --- | --- | --- | --- | --- |
| Duration | Batt A Voltage | Batt B Voltage | Batt C Voltage | Passing Criteria | Pass / Fail |
| 30 minutes |  |  |  | Only lowest charging |  |
| 60 minutes |  |  |  | Only lowest charging |  |
| 90 minutes |  |  |  | Only lowest charging |  |

## Battery Protection

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in Protection Circuits.

### Overcharge

#### Test Instructions

Charge or discharge the batteries to before this test. For each battery, apply a source to the input while increasing voltage until COUT transitions low. Remove the source and apply a resistive load until COUT transitions high again. Measure the battery voltage, COUT, and DOUT. Ensure the external control switches are configured to the correct battery.

Note: The overvoltage protection delay is typically 1.25s

#### Test Data

| Apply a source to the umbilical input with an increasing voltage until COUT transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery voltage, COUT, DOUT | Trigger Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  |  |
| B |  |  |  |  |
| C |  |  |  |  |

| During overvoltage protection, apply a resistive load until COUT transitions high | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery voltage, COUT, DOUT | Trigger Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  |  |
| B |  |  |  |  |
| C |  |  |  |  |

### Over-discharge

#### Test Instructions

Charge or discharge the batteries to before this test. For each battery, apply a resistive load to VBATT until DOUT transitions low. Remove the load and apply a source to the input until DOUT transitions high again. Measure the battery voltage, COUT, and DOUT. Ensure the external control switches are configured to the correct battery.

Note: The undervoltage protection delay is typically 144ms

#### Test Data

| Apply a resistive load to VBATT until DOUT transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery voltage, COUT, DOUT | Trigger Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  |  |
| B |  |  |  |  |
| C |  |  |  |  |

| During undervoltage protection, apply a source to the umbilical input until DOUT transitions high | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery voltage, COUT, DOUT | Trigger Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  |  |
| B |  |  |  |  |
| C |  |  |  |  |

### Charge Overcurrent

#### Test Instructions

Charge or discharge the batteries to before this test. For each protection circuit, insert the battery apply a source to the power inputs with increasing current until COUT transitions low. Decrease the current until COUT transitions high again. Measure the battery current, COUT, and DOUT. Ensure the external control switches are configured to the correct battery.

Note: Connect all the power inputs together to share the overcurrent.

#### Test Data

| Apply a source to the power inputs with an increasing current until COUT transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery current, COUT, DOUT | Trigger Current | Passing Criteria | Pass / Fail |
| A |  |  |  |  |
| B |  |  |  |  |
| C |  |  |  |  |

| Decrease the current from the previous source until COUT transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery current, COUT, DOUT | Trigger Current | Passing Criteria | Pass / Fail |
| A |  |  |  |  |
| B |  |  |  |  |
| C |  |  |  |  |

### Discharge Overcurrent

#### Test Instructions

Charge or discharge the batteries to before this test. For each protection circuit, insert the battery and apply an increasing load to VBATT until DOUT transitions low. Decrease the load until DOUT transitions high again. Measure the battery current, COUT, and DOUT. Ensure the external control switches are configured to the correct battery.

Note: Connect all the power outputs together to share the overcurrent.

#### Test Data

| Apply an increasing load to PR\_BATT outputs until DOUT transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery current, COUT, DOUT | Trigger Current | Passing Criteria | Pass / Fail |
| A |  |  |  |  |
| B |  |  |  |  |
| C |  |  |  |  |

| Decrease a high load on PR\_BATT outputs until DOUT transitions high | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Battery | Capture battery current, COUT, DOUT | Trigger Current | | Passing Criteria | | | Pass / Fail |
| A |  |  | |  | | |  |
| B |  |  | |  | | |  |
| C |  |  | |  | | |  |
| B |  | |  | |  |  | |

### Load Short Circuit

#### Test Instructions

Charge or discharge the batteries to before this test. For each protection circuit, insert the battery and apply a short between VBATT until DOUT. Then remove this short and measure the battery current, COUT, and DOUT. Ensure the external control switches are configured to the correct battery.

#### Test Data

| Apply a short between VBATT and PGND | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery current, COUT, DOUT | Trigger Delay | Passing Criteria | Pass / Fail |
| A |  |  |  |  |
| B |  |  |  |  |
| C |  |  |  |  |

| Remove the short between VBATT and PGND | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture battery current, COUT, DOUT | Trigger Delay | Passing Criteria | Pass / Fail |
| A |  |  |  |  |

## USB to UART Programming

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in USB to UART.

### Test Instructions

Connect a 5V 3A USB-C wall adapter to the board with all switches on. Upload a test code to the PENIC to turn on an LED and communicate information back.

### Test Data

| Upload code through the USB to UART converter | | |
| --- | --- | --- |
| Code Uploaded | Passing Criteria | Pass / Fail |
|  | LED turns on |  |
|  | Communication achieved |  |

### Test Notes

Replace this text with the test code used.

## Temperature Monitoring

**Results: Pass/Fail  
Configuration: Battery Charger V1.0.0**

This test evaluates the circuit described in PENIC and 3.3V Voltage Regulation.

### Test Instructions

Upload a test code to the PENIC to read the temperature from each thermistor voltage divider. Use either serial communication with the PENIC, or the LEDs for visual feedback. Use hot air to validate the voltage changes with temperature.

### Test Data

| Upload code for reading the thermistor voltages | | | |
| --- | --- | --- | --- |
| Thermistor | Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  |
| B |  |  |  |
| C |  |  |  |

### Test Notes

Replace this text with the test code used.

1. [LTC4411](https://www.analog.com/media/en/technical-documentation/data-sheets/4411fa.pdf) (Page 7) [↑](#footnote-ref-1)
2. [LED truth table](https://github.com/CougsInSpace/Resources/blob/master/Subsystems/Electronics/Testing/battery-charger/Documentation/IO_pins_truth_table.xlsx) [↑](#footnote-ref-2)
3. [BQ24650](https://github.com/CougsInSpace/Resources/blob/master/SupplierDocuments/60%20-%20Power%20IC/60-0008/TI_bq24650.pdf) [↑](#footnote-ref-3)
4. [NCR168650B](https://github.com/CougsInSpace/Resources/blob/master/SupplierDocuments/01%20-%20Battery/01-0002/NCR18650B.pdf) [↑](#footnote-ref-4)
5. [LTC4411](https://www.analog.com/media/en/technical-documentation/data-sheets/4411fa.pdf) [↑](#footnote-ref-5)
6. [BQ27900](https://github.com/CougsInSpace/Resources/blob/master/SupplierDocuments/60%20-%20Power%20IC/60-0006/TI_bq2971.pdf) [↑](#footnote-ref-6)
7. [CP2102N](https://www.silabs.com/documents/public/data-sheets/cp2102n-datasheet.pdf) [↑](#footnote-ref-7)
8. [PCB ARTISTS diagram](https://pcbartists.com/design/esp32-cp2102-programmer-schematic/) [↑](#footnote-ref-8)
9. [ESP32-S2-MINI-1](https://www.espressif.com/sites/default/files/documentation/esp32-s2_datasheet_en.pdf) [↑](#footnote-ref-9)
10. [LD1117A](https://www.digikey.com/en/htmldatasheets/production/8783/0/0/1/ld1117xx.html) [↑](#footnote-ref-10)
11. [NTCS0603E3T](https://github.com/CougsInSpace/Resources/blob/master/SupplierDocuments/26%20-%20Resistor%20Misc/26-0008/VISHAY_ntcs0603e3t.pdf) [↑](#footnote-ref-11)
12. [SK6812](https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf) [↑](#footnote-ref-12)
13. [Hackaday - level shifters](https://hackaday.com/2016/12/05/taking-it-to-another-level-making-3-3v-and-5v-logic-communicate-with-level-shifters/) [↑](#footnote-ref-13)
14. [Electronics Hub – level shifters](https://www.electronicshub.org/bidirectional-logic-level-converter/) [↑](#footnote-ref-14)